Flight Under:	Part 107	COA
SECTION 1 – Flight Information
Location:	Aircraft:
Remote Pilot in Charge (RPIC):	Flight Date:
Visual Observer(s):
SECTION 2 – Inspection Checklist
Flight Planning (Office)	Pre-Flight Checks (continued)
Check Weather Forecast	Calibrate Compass if Prompted
Check Airspace and NOTAMs	Confirm Max Altitude (120m/394ft)
File VAFIX	Confirm Max Distance (800m/2624ft)
File NOTAM (IGNIS use)	Confirm RTH Altitude (75m/246ft)
Obtain Airspace Clearance (if needed)	Confirm RTH if Signal Lost
Check Aircraft	Confirm Camera Set to Auto
Charge Aircraft Batteries	Format SD Card
Install SD Card	Check Weather Conditions
Charge Remote Control Battery	Check Surroundings
Charge iPad	Flight
Update Aircraft Firmware (optional)	Take Off
Update DJI Go 4 App (optional)	Set Precise RTH Location
Update DJI Geo-Fence (optional)	Confirm Joystick Control
Update Mapping Software (optional)	Confirm Camera Operation
Create Mapping Flight Plan (if needed)	Conduct Flight
Download Offline Map (if needed)	Maintain VLOS
On-Site Preparation	Maintain Communication with VO
Contact Landowner (if possible)	Monitor Aircraft Status
Confirm Weather Conditions for Flight	Monitor Remote Control Signal Strength
Check Area for Potential Hazards	Monitor GPS Satellite Coverage
Identify Take Off Site	Monitor Battery
Identify Visual Observer Positions	Complete Flight
Conduct Crew Briefing	Return to Home
Pre-Flight Checks	Land
Confirm Registration Number is Visible	Post Flight
Check Airframe	Power Off Aircraft
Check Motors and Install Propellers	Close DJI Go 4 App
Check IR and Visual Sensors	Power Off Remote Control
Remove Gimbal Clamp and Foam	Check Camera and Install Gimbal Guards
Check Camera and Clean Lens	Remove, Check and Clean Propellers
Confirm SD Card is Installed	Check and Clean Motors
Check Aircraft Battery	Check and Clean IR and Visual Sensors
Install iPad and Cable on Remote Control	Check and Clean Airframe
Verify Remote Control Mode is P	Confirm Registration Number Visible
Extend Remote Control Antenna	Remove iPad from Remote Control
Power on Remote Control	Fold Remote Antenna and iPad Holder
Open DJI Go 4	Pack Aircraft, Remote, Tablet, Etc.
Confirm No Other Apps Open	Flight Wrap-Up (Office)
Power on Aircraft	Copy/Backup Photos and Video
Connect DJI Go to Aircraft	Sync Flight Log to DJI and /or Airdata
Confirm Aircraft Status	File Flight Checklist
SECTION 3 – Inspected By
Remote Pilot in Charge Name (Print)	Remote Pilot in Charge Signature	Date