SECTION 1 – Equipment Information
Employee Name Equipment is Assigned To:	Inspection Date:
Truck (Year/Type):	Mileage:
SECTION 2 – Inspection Checklist
Item	Item
Fire Rakes (5)	Reflector Kit
Pulaski (1)	Credit Cards (Voyager & VDOT)
Shovel (1)	Tires Properly Inflated
Back Pack Tank or Bladder Bag	All Fuel Oil or Mix Containers Properly Labeled
Drip Torch with Fuel or Fusees	Boxes Clean
Water in Tank (if not below freezing)	Exterior Clean
Foam	Interior Clean
Chain Saw	Exterior Lights Operational
Chain Saw Chaps	Red Light Operational
Hand Lantern or Mag Light	Sirens Operational
Tow Chain	Winch Operational
Jack/Tire Iron	Spare Key in Place (in rear of driver side tool box)
Spare Tire	Hose, Suction, 2 ½” x 8’ (2)
Hand Tools (minimum- adj. Wrench, screw driver, pliers)	Adapter, Suction, 6” x 2 ½”
Fire Extinguisher	Foot Valve/Strainer, 2 ½”
Jumper Cables	Hose Shut-off Clamp
First Aid Kit	Hydrant Wrench
Gazetteer	Valve, 1 ½” Check/Bleeder
DOF/Local Directory	Valve, Shut-off, 1”
Tee, Inline with Valve, 1 ½” (2)	Valve, Shut-off, 1 ½”
Reducer, 1 ½” – 1” (2)	Valve, Gated Wye, 1 ½” (2)
Reducer, 1” – ¾” (2)	Valve, Shut-off, ¾” (2)
Increaser, ¾” – 1”	Wye, Plain, ¾” (2)
Increaser, 1” – 1 ½”	Nozzle, Barrel, 1 ½” (3)
Adapter, NH-NPSH, 1 ½”	Nozzle, Barrel, 1”
Adapter, NPSH-NH, 1 ½”	Nozzle, Forester, 1”
Coupling, Double Fem., 1 ½”	Nozzle, ¾” Garden Hose (2)
Coupling, Double Male, 1 ½”	Nozzle, 1 ½” Foam, 60gpm
Hose, 1” x 100’ (5)	Nozzle, 1” Foam, 18gpm (2)
Hose, 1 ½” x 100’ (5)	Nozzle, ¾” Foam, 8gpm
Hose, ¾” x 50’ (5)
In Case of Accident Information
Vehicle User Manual
Vehicle/Equipment Maintenance Record (updated)
Organization of Tool and Equipment:	Excellent	Good	Fair	Poor
Comments:
SECTION 3 – Inspected By
Inspector Name (Print)	Inspector Signature	Date