|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| SECTION 1 – Equipment Information | | | | | | | | | | | | | | | | |
| Employee Name Equipment is Assigned To: | | | | |  | | | | | | | Inspection Date: | | |  | |
| Truck (Year/Type): | | |  | | | | | | | | | Hours: | | |  | |
|  | | | | | | | | | | | | | | | | |
| SECTION 2 – Inspection Checklist | | | | | | | | | | | | | | | | |
|  | Item | | | | | | | |  | | Item | | | | | |
|  | Fire Shelters in Cab (2) | | | | | | | |  | |  | | | | | |
|  | Drip Torch with Fuel or Fusees | | | | | | | |  | |  | | | | | |
|  | Water or Foam in Tank (if not below freezing) (if equipped) | | | | | | | |  | |  | | | | | |
|  | Fire Extinguisher (if no water/foam system) | | | | | | | |  | |  | | | | | |
|  | Spare Hydraulic Hose for Fire Plow (plugged?) | | | | | | | |  | |  | | | | | |
|  | Axe | | | | | | | |  | |  | | | | | |
|  | Short Handle Shovel | | | | | | | |  | |  | | | | | |
|  | Track Pinch Bar | | | | | | | |  | |  | | | | | |
|  | Hammer | | | | | | | |  | |  | | | | | |
|  | Open End Wrenches | | | | | | | |  | |  | | | | | |
|  | Adjustable Wrench | | | | | | | |  | |  | | | | | |
|  | Screwdriver | | | | | | | |  | |  | | | | | |
|  | Wire Cutters | | | | | | | |  | |  | | | | | |
|  | Locking Vice Grip Pliers | | | | | | | |  | |  | | | | | |
|  | Fencing Pliers | | | | | | | |  | |  | | | | | |
|  | Vehicle User Manual | | | | | | | |  | |  | | | | | |
|  | Vehicle/Equipment Maintenance Record (updated) | | | | | | | |  | |  | | | | | |
|  | Tractor Starts | | | | | | | |  | |  | | | | | |
|  | Tractor Fully Fueled | | | | | | | |  | |  | | | | | |
|  | Hydraulic Oil at Proper Level | | | | | | | |  | |  | | | | | |
|  | Exterior Clean (free from debris) | | | | | | | |  | |  | | | | | |
|  | No Debris beneath Engine | | | | | | | |  | |  | | | | | |
|  | Interior Clean (free from debris) | | | | | | | |  | |  | | | | | |
|  | Exterior Night Lights Operational | | | | | | | |  | |  | | | | | |
|  | Spare Key in Place (with Transport Spare Key) | | | | | | | |  | |  | | | | | |
|  | Backup Alarm | | | | | | | |  | |  | | | | | |
|  | King Radio (in tractor or in transport) | | | | | | | |  | |  | | | | | |
|  | Radio Head-Set (in tractor or in transport) | | | | | | | |  | |  | | | | | |
|  | Seat-belt Mechanism Working Properly | | | | | | | |  | |  | | | | | |
|  | | | | | | | | | | | | | | | | |
| Organization of Tool and Equipment: | | | | Excellent | | | | Good | | Fair | | | Poor | | | |
| Comments: | |  | | | | | | | | | | | | | | |
|  | |  | | | | | | | | | | | | | | |
|  | |  | | | | | | | | | | | | | | |
|  | | | | | | | | | | | | | | | | |
| SECTION 3 – Inspected By | | | | | | | | | | | | | | | | |
|  | | | | | |  |  | | | | | | |  | |  |
| Inspector Name (Print) | | | | | |  | Inspector Signature | | | | | | |  | | Date |