Property No.:	Model:	Serial No.:	ESN No.:
Prevent. Mainten. Item	Description of Service	Notes:
Every 10 Hours or 12 Months	Date
Initials
Engine Oil	Check engine oil level with dipstick	Hours
Air Cleaner	Check/replace engine air filter element(s) & clean dust unloader valve
Radiator	Check coolant level in surge tank
Hydraulic/Hydrostatic Systems	Check fluid level
Fuel System	Check/drain fuel filter(s) & water separator
Cutting Edges, Plow Bolts	Check cutting edge condition & fastener tightness
Tracks	Check and adjust track sag to specifications
Winch	Check lubricant level, lubricate fairlead rollers, inspect cable, hook & chain
Lubricate	Dozer linkage, blade socket, adjustable pitch link, all grease fittings
Every 24 Months	Date
Initials
Perform PM	VDOF Shop completes 10-hour/12-month service	Hours
Clean & Inspect	Drop belly pans, clean & inspect for fluid leakage, clean under track frame covers
Engine Oil	Sample engine oil
Initial Service – 250 Hours or 6 Years	Date
Initials
Clean & Inspect	VDOF Shop completes 10-hour/12-month service	Hours
Engine Oil & Filter	Change break-in oil & replace filter
Every 250 Hours After Initial Service	Date
Initials
Engine Oil	Take engine oil sample	Hours
Final Drives	Check oil level
Fuel System	Drain final fuel filter sediment
Blade	Check & adjust blade pivot clearance
Every 500 Hours or 10 Years	Date
Initials
Engine Oil	Change oil/replace engine oil filter	Hours
Fuel System	Replace fuel filter(s)
Winch (if equipped)	Replace winch oil filter
Hydraulic/Hydrostatic Systems	Take fluid sample
Coolant/Antifreeze	Take coolant sample
Battery(ies)	Check water level, clean & tighten terminals
Belts & Hoses	Replace
Every 750 Hours or 15 Years	Date
Initials
Engine	Clean crankcase vent tube	Hours
Final Drives	Change lubricant
Coolant/Antifreeze	Check freeze protection
Engine Air Cleaner	Replace air cleaner filter element(s) & clean dust unloader valve
Winch (if equipped)	Change oil & filter, replace hydraulic reservoir breather filter

Property No.:	Model:	Serial No.:	ESN No.:
Prevent. Mainten. Item	Notes:
Every 10 Hours or 12 Months	Date
Initials
Engine Oil	Hours
Air Cleaner
Radiator
Hydraulic/Hydrostatic Systems
Fuel System
Cutting Edges, Plow Bolts
Tracks
Winch
Lubricate
Every 24 Months	Date
Initials
Perform PM	Hours
Clean & Inspect
Engine Oil
Initial Service – 250 Hours or 6 Years	Date
Initials
Clean & Inspect	Hours
Engine Oil & Filter
Every 250 Hours After Initial Service	Date
Initials
Engine Oil	Hours
Final Drives
Fuel System
Blade
Every 500 Hours or 10 Years	Date
Initials
Engine Oil	Hours
Fuel System
Winch (if equipped)
Hydraulic/Hydrostatic Systems
Coolant/Antifreeze
Battery(ies)
Belts & Hoses
Every 750 Hours or 15 Years	Date
Initials
Engine	Hours
Final Drives
Coolant/Antifreeze
Engine Air Cleaner
Winch (if equipped)