Property No.:	Model:	Serial No.:	ESN No.:
Prevent. Mainten. Item	Description of Service	Notes:
Every 10 Hours or 12 Months	Date
Initials
Engine Oil	Check engine oil level with dipstick	Hours
Air Cleaner Unloader Valve	Empty dust cap (if equipped)
Radiator/Surge Tank	Check coolant level
Hydraulic System	Check fluid level(s)
Transmission/Hydrostatic Sys.	Check fluid level(s)
Fuel System	Drain water
Cutting Edges/ Plow Bolts/ Plow Bearing Boxes	Check condition & fastener tightness
Grease Fittings	Lubricate all fittings
Tracks	Check and adjust track sag to specifications
Every 100 Hours or 12 Months	Date
Initials
Battery(ies)	Check water level & clean connections	Hours
Blade & Plow Control	Lubricate pivot points (G-Series Only)
Every 200 Hours or 24 Months	Date
Initials
Engine Oil & Filter	Change oil/replace engine oil filter	Hours
Air Filter	Replace only (do not clean)
Fuel Filter(s)	Replace
Clean & Inspect	Drop belly pans, clean & inspect for fluid leakage, clean under track frame covers
Every 500 Hours or 10 Years	Date
Initials
Transmission/Hydrostatic Sys.	Change fluid(s) & replace filter(s)	Hours
Coolant/Antifreeze	Drain & refill
Belts & Hoses	Replace
Final Drives	Drain & refill

Property No.:	Model:	Serial No.:	ESN No.:
Prevent. Mainten. Item	Notes:
Every 10 Hours or 12 Months	Date
Initials
Engine Oil	Hours
Air Cleaner Unloader Valve
Radiator/Surge Tank
Hydraulic System
Transmission/Hydrostatic Sys.
Fuel System
Cutting Edges/ Plow Bolts/ Plow Bearing Boxes
Grease Fittings
Tracks
Every 100 Hours or 12 Months	Date
Initials
Battery(ies)	Hours
Blade & Plow Control
Every 200 Hours or 24 Months	Date
Initials
Engine Oil & Filter	Hours
Air Filter
Fuel Filter(s)
Clean & Inspect
Every 500 Hours or 10 Years	Date
Initials
Transmission/Hydrostatic Sys.	Hours
Coolant/Antifreeze
Belts & Hoses
Final Drives