Instructions: Forklifts will be inspected prior to operating on any one day (see pre-use inspection checklist on how to conduct the inspection). The first operator of the day will complete the inspection. The operator should record the results of that inspection on the monthly pre-use inspection log so that other potential drivers that day can check the machine’s condition. On the line appropriate to the day of use, the operator will record how many hours are on the machine, if the machine passed or failed inspection, and if locked and tagged out, the reasons why. The monthly log should be kept on the machine during the applicable month, or in a location readily accessible to other operators.
Month:	Year:
SECTION 1 – Forklift Information
VIN/Vehicle Description:	Vehicle Location:
SECTION 2 – Monthly Pre-use Inspection Log
Day	Time	Hours on Machine	Inspector Name (please print)	Unit Passed Inspection	Unit Failed Inspection – Locked/ Tagged Out	If unit failed inspection, why? Or, attach pre-use inspection checklist and note in box below.
1
2
3
4
5
6
7
8
9
10
11
12
13
14
15
16
17
18
19
20
21
22
23
24
25
26
27
28
29
30
31